#
#  entries defining the dns root.  these will be overridden by any
#  authentic info obtained from the root.
#
dom=
	ns=A.ROOT-SERVERS.NET
	ns=B.ROOT-SERVERS.NET
	ns=C.ROOT-SERVERS.NET
	ns=D.ROOT-SERVERS.NET
	ns=E.ROOT-SERVERS.NET
	ns=F.ROOT-SERVERS.NET
	ns=G.ROOT-SERVERS.NET
	ns=H.ROOT-SERVERS.NET
	ns=I.ROOT-SERVERS.NET
	ns=J.ROOT-SERVERS.NET
	ns=K.ROOT-SERVERS.NET
	ns=L.ROOT-SERVERS.NET
	ns=M.ROOT-SERVERS.NET
dom=A.ROOT-SERVERS.NET ip=198.41.0.4
dom=B.ROOT-SERVERS.NET ip=128.9.0.107
dom=C.ROOT-SERVERS.NET ip=192.33.4.12
dom=D.ROOT-SERVERS.NET ip=128.8.10.90
dom=E.ROOT-SERVERS.NET ip=192.203.230.10
dom=F.ROOT-SERVERS.NET ip=192.5.5.241
dom=G.ROOT-SERVERS.NET ip=192.112.36.4
dom=H.ROOT-SERVERS.NET ip=128.63.2.53
dom=I.ROOT-SERVERS.NET ip=192.36.148.17
dom=J.ROOT-SERVERS.NET ip=198.41.0.10
dom=K.ROOT-SERVERS.NET ip=193.0.14.129
dom=L.ROOT-SERVERS.NET ip=198.32.64.12	# old
			ip=199.7.83.42	# new, nov 2007
dom=M.ROOT-SERVERS.NET ip=202.12.27.33


#  select one of the following two entries:

#
#  your domain if you are a dns server for your domain
#
dom=myuniversity.edu soa=
	refresh=3600 ttl=3600
	ns=ns1.myuniversity.edu
	ns=ns2.myuniversity.edu
	mx=mail.myuniversity.edu pref=1
	mx=mailbackup.myuniversity.edu pref=2
	mbox=netmaster@myuniversity.edu

#
#  your domain if you aren't a domain server for the domain
#
dom=myuniversity.edu
	ns=ns1.myuniversity.edu
	ns=ns2.myuniversity.edu

#
#  define your network.  dns, ntp, time, and wins are servers that can
#  be returned by dhcp. auth and fs are the default plan9 authentication
#  and name servers.  change the addresses to whatever makes sense in your
#  world.
#
#  each dnsdomain is a domain to search through when resolving
#  dnsnames
#
ipnet=mynetwork ip=10.0.0.0 ipmask=255.0.0.0
	fs=myfileserver.myuniversity.edu
	auth=myauthserver.myuniversity.edu
	dns=10.0.0.1
	dns=10.0.0.2
	wins=10.0.0.3
	wins=10.0.0.4
	ntp=10.0.0.5
	ntp=10.0.0.6
	time=10.0.0.7
	dnsdomain=cs.myuniversity.edu
	dnsdomain=ee.myuniversity.edu
	dnsdomain=math.myuniversity.edu
	dnsdomain=myuniversity.edu

#
#  a subnet of of your network.  you can override anything specified for the
#  network.
#
ipnet=mysubnetwork ip=10.0.1.0 ipmask=255.255.255.0
	dns=10.0.1.1
	dns=10.0.1.2

#
#  define a few systems.  if they support the il protocol, say so.  otherwise
#  the connection server will assume they just know tcp and udp.
#	- the sys= tuple specifies a local nickname for the machine.
#	- unless a bootf= tuple exists, dhcp will not answer boot requests for it
#
ip=10.0.1.10 ether=0010dc724074 sys=fs
	dom=myfileserver.myuniversity.edu 
	bootf=/386/9boot			# to load /386/9pcfs

ip=10.0.1.11 ether=0010dc724075 sys=auth
	dom=myauthserver.myuniversity.edu
	bootf=/386/9boot			# to load /386/9pccpu

ip=10.0.1.12 ether=0010dc724076 sys=term
	dom=myterminal.myuniversity.edu
	bootf=/386/9boot			# to load /386/9pc

auth=sources.cs.bell-labs.com authdom=outside.plan9.bell-labs.com
